[image: d20156129636286.gif]5" Fireproof Ceiling Speaker (3W-6W)                                                                                      
FFS-305                                                                                                                                                                                                                                                                    

Feature:
· Commercial fireproof ceiling speaker with transformer.
· Ideal for school, office, hotel and airport voice evacuation and PA system.
· Compliant with the EN54-24 EVAC standard.
· Ceramic connector, fire dome, 95℃ fire-resistant cable and thermal fuse.
· Rated power output 3W-6W at 100V.
· 5" full range paper woofer.
· [bookmark: _GoBack]Line input 100V or 70V with transformer.
· With A/B two speaker cable entry.
· Metal enclosure, metal grille in white and fire dome in red.
· In-ceiling quick installation by spring clip.

Specification:
	Model
	FFS-305

	Description
	5” Fireproof Ceiling Speaker

	Rated Power Output
	3W-6W

	Line Input
	100V or 70V

	Frequency Response
	130-15KHz

	SPL(@1W/m)
	92dB

	Speaker Unit
	5” full range paper woofer

	Cutout Size
	160mm

	Dimension
	180(D)×135(H)mm

	Material
	Metal enclosure, metal grille in white and fire dome in red

	Mounting Way
	In-ceiling spring clip quick installation

	Weight
	1.3kg
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Frequency Response & SPL Diagram:
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